**Jigsaw – Instructions for use**

**PRE-START CHECKs:**

* Ensure switch is in the off position before connecting to the power supply.
* Inspect workpiece for any nails & remove them before operation.

**OPERATION:**

* The first thing you will want to do is to clamp your board down.
* Remember to leave space underneath your piece so that there is room for the blade to move.
* Plug in to power supply.
* Place the front of the shoe on the edge of your material. Start the saw with the blade **OFF**the material, then slowly bring the blade to the edge and begin your cut.
* Let the saw come to a complete stop before lifting the blade out of the wood.

**STOPPING AND AFTER USE:**

* Push switch to off position.
* Turn off power supply & unplug machine.
* Dust machine off.

**SAFETY PRECAUTIONS:**

* Always switch off & wait for the blade to come to a complete stop before removing the blade.
* Do not touch the blade or workpiece immediately after use – they may be extremely hot.

**REQUIRED SAFETY EQUIPMENT:**

****

 

