**Pencil Vibrator (small electric) – Instructions for use**

**PRE-START CHECKS:**

* Check the area of operation for hazards.
* Make sure the unit is switched off before connection to the power supply.
* Make sure the flexi shaft & head are connected securely.

**OPERATION:**

* Plug the unit into the power source.
* Turn on the power source.
* Turn on the concrete vibrator.
* Ensure unit is held in a secure manner while operating.

**STOPPING AND AFTER USE:**

* Turn off the concrete vibrator.
* Turn off the power source.
* Unplug the unit.
* Make sure the unit is cleaned of excess concrete.
* Avoid water on the motor & electrical components.

**SAFETY PRECAUTIONS:**

* Only switch on when ready to use in concrete.
* Switch off immediately after removing from concrete.
* Always ensure a steady stance & control of the unit.

**REQUIRED SAFETY EQUIPMENT:**

****

